------------------------------------------------

Low Level Design Document for Device

Driver For a Simulated Character Device

Table of contents: 1 to 2

1. Introduction ……………………………………………………………………...

1.1 Purpose …………………………………………………………………

1.2 Document Conventions …………………………………………..

* 1. Intended Audience and Reading Suggestions ………………
  2. References …………………………………………………………….

2 to 3

1. System Use cases ……………………………………………………………….

3 to 16

3 Detailed System Design …………………………………………………………

3.1 Kernel mode …………………………………………………………

3.2 User ………………………………………………………………….…

3.3 IOCTL ………………………………………………………………….

3.4 Interface between kernel and user …………………………..

3.5 Hardware communication ………………………………………

16 to 17

4 Security …………………………………………………………………………….…

1. **Introduction:-**

1.1 **Purpose:**

In LINUX, hardware devices are accessed by the user through special device files. These files are grouped into the /dev directory, and system calls open, read, write, close, lseek, mmap etc. are redirected by the operating system to the device driver associated with the physical device. The device driver is a kernel component (usually a module) that interacts with a hardware device.

In the LINUX world there are two categories of device files and thus device drivers: character and block. This division is done by the speed, volume and way of organizing the data to be transferred from the device to the system and vice versa. In the first category, there are slow devices, which manage a small amount of data, and access to data does not require frequent seek queries. Examples are devices such as keyboard, mouse, serial ports, sound card, joystick. In general, operations with these devices (read, write) are performed sequentially byte by byte. The second category includes devices where data volume is large, data is organized on blocks, and search is common. Examples of devices that fall into this category are hard drives, cdroms, ram disks, magnetic tape drives. For these devices, reading and writing is done at the data block level.

For the two types of device drivers, the Linux kernel offers different APIs. If for character devices system calls go directly to device drivers, in case of block devices, the drivers do not work directly with system calls. In the case of block devices, communication between the user-space and the block device driver is mediated by the file management subsystem and the block device subsystem. The role of these subsystems is to prepare the device driver's necessary resources (buffers), to keep the recently read data in the cache buffer, and to order the read and write operations for performance reasons.

1.2 **Documents conversions**:

TBD.

1.3 **Intended Audience and Reading Suggestions**:

Document is primarily intended for members of LDD team which consists of graduate students working under the guidance of Mr. Sweatank.

1.4 **References:**

Project proposal document

System specification of IOCTL

System architecture and high-level design of IOCTL

2. **System Use Cases:**

The project involving a simulated character device with `ioctl` system use cases can serve various purposes, including:

1. \*\*Educational Purposes\*\*: It can be used as a learning tool for understanding device drivers, character devices, and `ioctl` system calls in the Linux kernel. Students studying operating systems or kernel development can use it to gain hands-on experience.

2. \*\*Testing and Debugging\*\*: Kernel developers and system administrators can use it for testing and debugging purposes. They can simulate different scenarios and test how the system behaves under various `ioctl` commands.

3. \*\*Prototyping and Development\*\*: It can be a starting point for prototyping new device drivers or experimenting with new features. Developers can build upon the basic framework to create custom device drivers tailored to specific hardware or software requirements.

4. \*\*Research and Experimentation\*\*: Researchers and hobbyists interested in kernel development can use it for experimentation and research purposes. They can explore different aspects of kernel programming, performance tuning, and system behaviour.

5. \*\*Integration with User Space Applications\*\*: Once the device driver is developed, it can be integrated into user space applications that require low-level access to hardware or system functionality. For example, it could be used in embedded systems, IoT devices, or specialized software applications.

Overall, the project provides a practical foundation for understanding and working with device drivers and kernel-level programming in the Linux environment.

3**. Deayled System Design**:

3.1 **Kernel mode:**

Source code:

#include <linux/init.h>

#include <linux/module.h>

#include <linux/fs.h>

#include <linux/uaccess.h>

#include <linux/cdev.h>

#define DEVICE\_NAME "my\_ioctl\_device"

#define IOCTL\_MAGIC 'k'

#define IOCTL\_SET\_STRING \_IOW(IOCTL\_MAGIC, 2, char \*)

#define IOCTL\_GET\_STRING \_IOR(IOCTL\_MAGIC, 3, char \*)

static char kernel\_string[100] = {0}; // Buffer to store string from user space

static int device\_open(struct inode \*inode, struct file \*file) {

printk(KERN\_INFO "Device opened\n");

return 0;

}

static int device\_release(struct inode \*inode, struct file \*file) {

printk(KERN\_INFO "Device closed\n");

return 0;

}

static long device\_ioctl(struct file \*file, unsigned int cmd, unsigned long arg) {

switch (cmd) {

case IOCTL\_SET\_STRING:

if (copy\_from\_user(kernel\_string, (char \_\_user \*)arg, sizeof(kernel\_string))) {

return -EFAULT;

}

printk(KERN\_INFO "String received: %s\n", kernel\_string);

break;

case IOCTL\_GET\_STRING:

if (copy\_to\_user((char \_\_user \*)arg, kernel\_string, sizeof(kernel\_string))) {

return -EFAULT;

}

printk(KERN\_INFO "String sent to user: %s\n", kernel\_string);

break;

default:

return -ENOTTY;

}

return 0;

}

static struct file\_operations fops = {

.owner = THIS\_MODULE,

.open = device\_open,

.release = device\_release,

.unlocked\_ioctl = device\_ioctl,

};

static int major\_number;

static struct cdev my\_cdev;

static int \_\_init my\_ioctl\_init(void) {

major\_number = register\_chrdev(0, DEVICE\_NAME, &fops);

if (major\_number < 0) {

printk(KERN\_ALERT "Registering char device failed with %d\n", major\_number);

return major\_number;

}

cdev\_init(&my\_cdev, &fops);

my\_cdev.owner = THIS\_MODULE;

if (cdev\_add(&my\_cdev, MKDEV(major\_number, 0), 1)) {

unregister\_chrdev(major\_number, DEVICE\_NAME);

printk(KERN\_ALERT "Adding cdev failed\n");

return -1;

}

printk(KERN\_INFO "Device registered with major number %d\n", major\_number);

return 0;

}

static void \_\_exit my\_ioctl\_exit(void) {

cdev\_del(&my\_cdev);

unregister\_chrdev(major\_number, DEVICE\_NAME);

printk(KERN\_INFO "Device unregistered\n");

}

module\_init(my\_ioctl\_init);

module\_exit(my\_ioctl\_exit);

MODULE\_LICENSE("GPL");

MODULE\_AUTHOR ("Your Name");

MODULE\_DESCRIPTION ("A simple Linux char driver with ioctl for string set/get");

MODULE\_VERSION ("0.1");

Explanation:

Kernel Code Documentation: my\_ioctl\_device.c

This code implements a simple character device driver named "my\_ioctl\_device" that allows user-space applications to interact with the kernel using ioctls (Input/Output Control) for setting and getting a string value.

**Functionality:**

* The driver creates a character device named "my\_ioctl\_device".
* User-space applications can open, close, and interact with the device using ioctls.
* Two ioctl commands are defined:
  + IOCTL\_SET\_STRING: Allows applications to set a string value in the kernel.
  + IOCTL\_GET\_STRING: Allows applications to get the current string value stored in the kernel.

**Code Breakdown:**

**Headers:**

* <linux/init.h>: Used for module initialization and exit functions.
* <linux/module.h>: Defines macros for module licensing, author, description, etc.
* <linux/fs.h>: Provides structures and functions related to the file system.
* <linux/uaccess.h>: Provides functions for safe data transfer between user and kernel space.
* <linux/cdev.h>: Provides structures and functions for character devices.

**Constants:**

* DEVICE\_NAME: Name of the character device ("my\_ioctl\_device").
* IOCTL\_MAGIC: Magic number used for constructing ioctl commands.
* IOCTL\_SET\_STRING: ioctl command for setting a string value (\_IOW macro).
* IOCTL\_GET\_STRING: ioctl command for getting a string value (\_IOR macro).

**Global Variable:**

* kernel\_string: Character array to store the string received from user space (size 100).

**File Operations:**

* device\_open: Opens the device and prints a message to the kernel log.
* device\_release: Closes the device and prints a message to the kernel log.
* device\_ioctl: Handles ioctl requests:
  + IOCTL\_SET\_STRING: Copies the string from user space to the kernel buffer, prints the received string to the kernel log.
  + IOCTL\_GET\_STRING: Copies the string from the kernel buffer to user space, prints the sent string to the kernel log.
  + Returns an error for unsupported commands.

**Module Initialization and Exit:**

* my\_ioctl\_init: Registers the character device, initializes the cdev structure, and adds the cdev to the system.
* my\_ioctl\_exit: Removes the cdev from the system and unregisters the character device.

**Module Information:**

* MODULE\_LICENSE: License information (GPL in this case).
* MODULE\_AUTHOR: Author name (r your name).
* MODULE\_DESCRIPTION: Description of the module functionality.
* MODULE\_VERSION: Version number of the module (0.1 ).

3.2 **User mode**:

Source code:

#include <stdio.h>

#include <stdlib.h>

#include <fcntl.h>

#include <unistd.h>

#include <sys/ioctl.h>

#define DEVICE\_PATH "/dev/my\_ioctl\_device"

#define IOCTL\_MAGIC 'k'

#define IOCTL\_SET\_STRING \_IOW(IOCTL\_MAGIC, 2, char \*)

#define IOCTL\_GET\_STRING \_IOR(IOCTL\_MAGIC, 3, char \*)

int main() {

int fd;

char user\_string[100]; // Buffer for string to kernel space

char kernel\_response[100]; // Buffer for string from kernel space

// Open the device

fd = open(DEVICE\_PATH, O\_RDWR);

if (fd < 0) {

perror("Failed to open the device");

return EXIT\_FAILURE;

}

// Set the string to the kernel

snprintf(user\_string, sizeof(user\_string), "Hello, Kernel!");

if (ioctl(fd, IOCTL\_SET\_STRING, user\_string) < 0) {

perror("Failed to send string to the kernel");

close(fd);

return EXIT\_FAILURE;

}

// Get the string from the kernel

if (ioctl(fd, IOCTL\_GET\_STRING, kernel\_response) < 0) {

perror("Failed to get string from the kernel");

close(fd);

return EXIT\_FAILURE;

}

printf("String received from the kernel: %s\n", kernel\_response);

// Close the device

close(fd);

return EXIT\_SUCCESS;

}

Explanation:

User Code Documentation: user\_ioctl.c

This code implements a user-space application that interacts with the my\_ioctl\_device character device driver using ioctls.

**Functionality:**

* The application opens the device named "/dev/my\_ioctl\_device".
* It sends a string ("Hello, Kernel!") to the kernel using the IOCTL\_SET\_STRING ioctl command.
* Then, it retrieves the current string value stored in the kernel using the IOCTL\_GET\_STRING ioctl command.
* Finally, it prints the received string to the standard output.

**Code Breakdown:**

**Headers:**

* <stdio.h>: Provides standard input/output functions (printf).
* <stdlib.h>: Provides general utility functions (exit, snprintf).
* <fcntl.h>: Provides file control constants (O\_RDWR).
* <unistd.h>: Provides standard POSIX functions (open, close, read, write, etc.).
* <sys/ioctl.h>: Provides functions for performing ioctls.

**Constants:**

* DEVICE\_PATH: Path to the character device ("/dev/my\_ioctl\_device").
* IOCTL\_MAGIC, IOCTL\_SET\_STRING, IOCTL\_GET\_STRING: Same as in the kernel code for consistency.

**User Buffers:**

* user\_string: Character array to store the string to be sent to the kernel (size 100).
* kernel\_response: Character array to store the string received from the kernel (size 100).

**Main Function:**

* Opens the device using open with read/write permissions.
* Uses snprintf to format the string "Hello, Kernel!" into the user\_string buffer.
* Calls ioctl to send the string to the kernel using IOCTL\_SET\_STRING.
* Calls ioctl again to get the string from the kernel using IOCTL\_GET\_STRING.
* Prints the received string from the kernel using printf.
* Closes the device using close.

3.3 **ioctl:-**

device-specific input/output operations and other operations which cannot be expressed by regular file semantics. It takes a parameter specifying a request code; the effect of a call depends completely on the request code. Request codes are often device-specific. For instance, a CD-ROM device driver which can instruct a physical device to In computing **ioctl** (an abbreviation of **input/output control**) is a system call for eject a disc would provide an ioctl request code to do so. Device-independent request codes are sometimes used to give user space access to kernel functions which are only used by core system software or still under development.

The ioctl system call first appeared in version 7 of unix under that name. It is supported by most Unix and unix-like systems, including linux and macOS though the available request codes differ from system to system. Microsoft windows provides a similar function, named "DeviceIoControl", in its win32api

Conventional operating systems can be divided into two layers, userspace and the kernel. Application code such as a text editor resides in userspace, while the underlying facilities of the operating system, such as the network stack reside in the kernel. Kernel code handles sensitive resources and implements the security and reliability barriers between applications; for this reason, user mode applications are prevented by the operating system from directly accessing kernel resources.

Userspace applications typically make requests to the kernel by means of system calls whose code lies in the kernel layer. A system call usually takes the form of a "system call vector", in which the desired system call is indicated with an index number. For instance, exit() might be system call number 1, and write() number 4. The system call vector is then used to find the desired kernel function for the request. In this way, conventional operating systems typically provide several hundred system calls to the userspace.

Though an expedient design for accessing standard kernel facilities, system calls are sometimes inappropriate for accessing non-standard hardware peripherals. By necessity, most hardware peripherals (aka devices) are directly addressable only within the kernel. But user code may need to communicate directly with devices; for instance, an administrator might configure the media type on an ethernet interface. Modern operating systems support diverse devices, many of which offer a large collection of facilities. Some of these facilities may not be foreseen by the kernel designer, and as a consequence it is difficult for a kernel to provide system calls for using the devices.

To solve this problem, the kernel is designed to be extensible, and may accept an extra module called a device driver which runs in kernel space and can directly address the device. An ioctl interface is a single system call by which userspace may communicate with device drivers. Requests on a device driver are vectored with respect to this ioctl system call, typically by a handle to the device and a request number. The basic kernel can thus allow the userspace to access a device driver without knowing anything about the facilities supported by the device, and without needing an unmanageably large collection of system calls.

Hardware design configuration:-

A common use of ioctl is to control hardware devices.

For example, on win32 systems, ioctl calls can communicate with usb devices, or they can discover drive-geometry information of the attached storage-devices.

On openbsd and netbsd, ioctl is used by the  pseudo-device driver and the bioctl utility to implement  raid volume management in a unified vendor-agnostic interface similar to iconfig.

On netBSD, ioctl is also used by the SYSMON  framework.

Kernel extansion:-

When applications need to extend the kernel, for instance to accelerate network processing, ioctl calls provide a convenient way to bridge userspace code to kernel extensions. Kernel extansion can provide a location in the filesystem that can be opened by name, through which an arbitrary number of ioctl calls can be dispatched, allowing the extension to be programmed without adding system calls to the operating system.

Syscall alternative:-

According to an open BSD developer, ioctl and sysctl are the two system calls for extending the kernel, with sysctl possibly being the simpler of the two.

In netBSD, the sysmon framework for hardware monitoring uses ioctl through proplib; whereas open BSD and dragon fly BSD instead use SYSCTL for their corresponding HW.sensors framework. The original revision of envsys in NetBSD was implemented with ioctl before proplib was available, and had a message suggesting that the framework is experimental, and should be replaced by a sysctl(8) interface, should one be developed, which potentially explains the choice of sysctl in OpenBSD with its subsequent introduction of  in 2003. However, when the  framework was redesigned in 2007 around proplib, the system call remained as ioctl, and the message was removed.

**Key aspects of ioctl:-**

1. **Usage and Syntax**:
   * The ioctl function prototype is: int ioctl(int fd, unsigned long request, ...).
   * **fd**: File descriptor of the device.
   * **request**: A command code indicating the operation to be performed.
   * **...**: Additional arguments, usually pointers to data structures or values.
2. **Command Codes**:
   * Command codes are unique to each device and defined by the driver developer. They are often created using macros to ensure uniqueness and proper encoding.
   * Example: #define IOCTL\_GET\_STATS \_IOR(MY\_MAGIC, 0, struct stats).
3. **Types of IOCTL Commands**:
   * **\_IOR**: Read data from the device.
   * **\_IOW**: Write data to the device.
   * **\_IOWR**: Read/write data from/to the device.
   * **\_IO**: Perform a simple command with no data transfer.
4. **Common Use Cases**:
   * Configuring device parameters.
   * Retrieving device status.
   * Sending control commands to hardware (e.g., ejecting a CD, formatting a disk).

int fd = open("/dev/mydevice", O\_RDWR);

if (fd == -1) {

perror("Failed to open device");

return errno;

}

struct stats device\_stats;

if (ioctl(fd, IOCTL\_GET\_STATS, &device\_stats) == -1) {

perror("Failed to get device stats");

return errno;

}

close(fd);

3.4 **inetrface between kernel and user:-**

The **interface between the kernel and user space** is a fundamental aspect of an operating system, providing the means for user applications to interact with the system's core functionality.

The Linux kernel provides multiple interfaces to user-space and kernel-mode code that are used for varying purposes and that have varying properties by design. There are two types of application programming interface (API) in the Linux kernel: the "kernel–user space" API; and. the "kernel internal" API.

Key components

**System Calls**:

System calls are the main interface between user applications and the kernel. They allow user programs to request services from the kernel, such as file operations, process control, and memory management. Examples include open, read, write, fork, and exec.

* + The primary interface for user programs to request services from the kernel.
  + Examples include file operations (open, read, write), process control (fork, exec), and memory management (mmap).

**Procfs and Sysfs**:

* + **Procfs** (/proc): A virtual filesystem that provides a mechanism to access kernel data structures. It includes information about processes, system configuration, and hardware.
  + **Sysfs** (/sys): Another virtual filesystem that exposes kernel objects, their attributes, and their relationships. It's used for device and driver information.

**IOCTL**:

IOCTL (Input/Output Control) is a system call used for device-specific operations not covered by standard system calls. It allows user-space applications to send control commands directly to device drivers. An example use is configuring device parameters or retrieving device-specific information.

* + As described above, IOCTL provides a way to perform device-specific operations not covered by standard system calls.

**Netlink**:

Netlink is a socket-based IPC mechanism used for communication between the kernel and user-space processes, particularly for networking-related operations. It is commonly used for network configuration and receiving notifications about kernel events.


* + A socket-based IPC mechanism used for communication between the kernel and user-space processes, particularly useful for networking operations and configuration.

**Debugfs**

Debugfs is a special-purpose filesystem for debugging kernel code, providing a way to expose internal kernel data structures and variables to user space. It is mounted at /sys/kernel/debug and is used primarily by developers for debugging purposes

**File system in user space(fuse)**

FUSE allows the creation of filesystems implemented in user space, providing flexibility and easier debugging for filesystem development. It enables user-space programs to implement a fully functional filesystem without modifying kernel code.

**Architecture of the kernel the user application interact:-** 

3.5 **Hardware communication:-**

In Linux, hardware communication is managed through a combination of device drivers, interrupt handling, memory-mapped I/O, Direct Memory Access (DMA), and standardized communication protocols. These mechanisms enable the operating system to interact efficiently and effectively with various hardware components.

**Device drivers:-**

**Device drivers** are kernel modules that act as intermediaries between the hardware and the operating system. They handle the specifics of hardware communication, providing a standardized interface for the OS to interact with different types of hardware devices.

* **Types of Device Drivers**:
  + **Character Drivers**: Handle devices that transmit data as a stream of characters (e.g., keyboards, serial ports).
  + **Block Drivers**: Manage devices that read/write data in blocks (e.g., hard drives, SSDs).
  + **Network Drivers**: Facilitate communication over network interfaces (e.g., Ethernet, Wi-Fi adapters).

**Interrupts:-**

**Interrupts** are signals sent by hardware devices to the CPU to indicate that they require immediate attention. When an interrupt occurs, the CPU stops its current activities to service the interrupt, allowing the device to communicate urgent information or request processing.

* **Types of Interrupts**:
  + **Hardware Interrupts**: Generated by hardware devices (e.g., pressing a key on the keyboard, network packet arrival).
  + **Software Interrupts**: Generated by software instructions to signal the kernel.
* **Interrupt Handling**:
  + The kernel has interrupt handlers (also known as Interrupt Service Routines, ISRs) that are registered to handle specific interrupts. When an interrupt is received, the corresponding ISR processes it.

**Memory-mapped i/o:-**

**Memory-Mapped I/O (MMIO)** is a method where the control registers of a hardware device are mapped into the system’s address space. This allows the CPU to interact with the hardware using standard memory instructions.

* **Advantages**:
  + Simplifies the interaction between the CPU and hardware.
  + Provides efficient data transfer between the CPU and device registers.
* **Implementation**:
  + Device registers are mapped to specific addresses in the memory space.
  + The kernel can read from or write to these addresses to control the hardware.

**Direct memory access:-**

**Direct Memory Access (DMA)** is a feature that allows hardware devices to transfer data directly to or from memory without involving the CPU. This enhances system performance by freeing the CPU from data transfer tasks and allowing it to perform other operations.

* **DMA Controller**:
  + Manages DMA operations and coordinates the data transfers between devices and memory.
  + Ensures that the data transfer occurs without conflicts and in an efficient manner.
* **Use Cases**:
  + High-speed data transfer operations (e.g., disk I/O, network data transfer).
  + Situations requiring minimal CPU intervention.

**Standard communication protocals**:-

**Standard communication protocols** are used for interfacing with various peripheral devices. These protocols ensure compatibility and standardized communication methods between the OS and hardware.

* **Common Protocols**:
  + **I2C (Inter-Integrated Circuit)**: Used for communication between integrated circuits.
  + **SPI (Serial Peripheral Interface)**: Used for short-distance communication, primarily in embedded systems.
  + **UART (Universal Asynchronous Receiver/Transmitter)**: Used for serial communication, such as with serial ports.
  + **PCI/PCIe (Peripheral Component Interconnect/Express)**: Used for connecting high-speed devices like graphics cards and network adapters.

4. **Security:-**

The user-to-kernel interfaces of mainstream operating systems are often audited heavily for code flaws and security vulnerabilities prior to release. These audits typically focus on the well-documented system call interfaces; for instance, auditors might ensure that sensitive security calls such as changing user IDs are only available to administrative users.

ioctl interfaces are more complicated, more diverse, and thus harder to audit than system calls. Furthermore, because ioctl calls can be provided by third-party developers, often after the core operating system has been released, ioctl call implementations may receive less scrutiny and thus harbor more vulnerabilities. Finally, many ioctl calls, particularly for third-party device drivers, are undocumented.

Because the handler for an ioctl call resides directly in kernel mode, the input from userspace should be validated carefully. Vulnerabilities in device drivers can be exploited by local users by passing invalid buffers to ioctl calls.

Win32 and unix operating systems can protect a userspace device name from access by applications with specific access controls applied to the device. Security problems can arise when device driver developers do not apply appropriate access controls to the userspace accessible object.

Some modern operating systems protect the kernel from hostile userspace code (such as applications that have been infected by buffer overflow exploits) using system calls waffers System call wrappers implement role base access control by specifying which system calls can be invoked by which applications; wrappers can, for instance, be used to "revoke" the right of a mail program to spawn other programs. ioctl interfaces complicate system call wrappers because there are large numbers of them, each taking different arguments, some of which may be required by normal programs.

**Key areas:-**

1. **Authentication and Authorization**:
   * **Authentication**: Verifying the identity of users (e.g., passwords, biometrics).
   * **Authorization**: Ensuring users have permission to access resources (e.g., file permissions, role-based access control).
2. **Encryption**:
   * Protecting data at rest and in transit using cryptographic techniques (e.g., AES, RSA).
   * Ensures data cannot be easily accessed or tampered with.
3. **Access Control**:
   * Implementing policies that define who or what can access certain resources.
   * Mechanisms include:
     + **File Permissions**: Read, write, and execute permissions for files and directories.
     + **Access Control Lists (ACLs)**: More granular permissions settings.
     + **Role-Based Access Control (RBAC)**: Assigning permissions based on user roles.
4. **Kernel Security**:
   * **Secure Boot**: Ensuring the system boots using trusted software.
   * **Kernel Lockdown**: Restricting certain kernel functionality to enhance security.
   * **Mandatory Access Control (MAC)**: Enforcing strict access policies using frameworks like SELinux or AppArmor.
5. **Audit and Logging**:
   * Keeping detailed logs of system activities to monitor and detect anomalies.
   * Important for forensic analysis in case of security incidents.
6. **Network Security**:
   * Protecting the system from network-based threats.
   * Tools and techniques include:
     + **Firewalls**: Filtering incoming and outgoing traffic based on rules.
     + **Intrusion Detection/Prevention Systems (IDS/IPS)**: Monitoring and responding to suspicious activities.
     + **Secure Communication Protocols**: Using protocols like SSL/TLS for secure data transmission.